**SPESIFIKASI**

**TOTAL STATION**

|  |  |
| --- | --- |
| Nama barang a) | **TOTAL STATION** |
| Merk | LEICA FELXILINE |
| Type/ model | Leica TS 07  |
| Persyaratan tambahan | Weight 9.5 to 9.9 lbs (4.3 to 4.5 kg)Dimensions 12.51” L x 8.81” W x 7.66” H (31.8 cm x 22.4 cm x 19.5 cm)Warranty 1-yearProtection Class IP66 dustproof and water jet resistantInternal Memory 2 GBSoftware FlexFieldTribrach N/AAngle MeasurementMeasuring Method/Reading System Absolute, continuous, diametricalAccuracy 1 second, 2 second, 3 second, 5 second, 7 secondDistance MeasurementUnit of Measure (distance display) m/ftEDM Accuracy (Precision) 1 mm + 1.5 ppm (typical 2.4 s)Tilt Sensor/CompensatorRange ±4 degreesType Quadruple-axisSetting Accuracy ±2″ / 3″ / 5″Battery/PowerPower Source Rechargeable Li-ion batteriesBattery Life Up to 30 hours (GEB361)Display and KeypadType 3.5″ LCD colored displaySides SingleKeys 28 keys, illuminatedTouchscreen YesBacklight YesPixels 320 x 240 pixels**Sudah Terkalibrasi KAN** |
| Jumlah | 1 Unit |
| Franco | Unit Pelayanan (UP) Ambon |

**Note:**

**Mohon dapat menyampaikan :**

* Surat Penawaran dengan harga yang sudah **Net**
* Harga sudah meliputi biaya pengiriman dengan franco **Ambon (Alamat PT SUCOFINDO Unit Pelayanan Ambon)**, Biaya Instalasi, Biaya Pelatihan dan Uji coba.
* Lampiran surat penawaran berupa spesifikasi detail.
* Penyedia Eksternal yang mengikuti pengadaan ini harus melampirkan sertifikat TKDN / surat pernyataan penggunaan komponen dalam negeri (TKDN)
* Pakta Integritas (dapat di down load pada link (<https://eproc.sucofindo.co.id/index.php/paktaintegritas> )

**Note: untuk menghindari kesalahan pada submit harga, kepada Bapak / Ibu agar dapat mendownload user manualnya pada link <https://eproc.sucofindo.co.id/index.php/usermanual> ) – Dokumen – User Manual**